1. Write an assembly language program to swap two 8-bit datausing 8085 processor.

LDA 2500

MOV B,A

LDA 2501

STA 2500

MOV A,B

STA 2501

HLT